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[bookmark: _Toc57301845][bookmark: _Toc216966729]1.	Information about plan's developer
Information about the developer and holder of the plan
The Yeisk branch of the Federal State Budgetary Institution "Administration of the Sea Ports of the Sea of Azov" (hereinafter - the Yeisk Branch of the FSBI "AMP of the Azov Sea") was established in accordance with the order of the Ministry of Transport of the Russian Federation dated 26.03.2015 No. 51 "On the reorganization of the Federal State Budgetary Institution" Administration of the seaports of the Azov Sea "in the form of joining the Federal State Institution" Administration of the Seaport of Yeysk ".
The Yeisk branch of the FSBI "AMP of the Sea of Azov" is a non-profit organization that, within its competence, provides state services in maritime transport in the field of organizing and ensuring the safety of navigation.
Ensuring the ecological safety of navigation and environmental protection is achieved by:
- organization and control of measures to prevent environmental pollution by wastes from ships;
- organizing the activities of receiving port facilities for waste from ships;
- organization of measures to eliminate emergency environmental pollution from ships.
Official name:
Federal State Budgetary Institution "Administration of the Sea Ports of the Sea of ​​Azov", Yeisk Branch
Address: 353680 Yeisk, st. Beach, 6;
Contacts: (86132) 2-61-27, fax. (86132) 2-06-24, maemp@mail.ru portcontroleysk@mail.ru

Head: Captain of the seaport of Yeysk G.V. Bulavin

The composition of the plan development team:
Konischev A.V., Moloshenko B.V.



[bookmark: _Toc57301846][bookmark: _Toc216966730]	2.	Terms and definitions
	Seaport water area
	Water space within the boundaries determined by the Compulsory Seaport Regulations

	Outer road
	Water space allocated and intended for anchorage and servicing of ships at anchor

	Sufficiency
	The sufficiency of resolution MEPC.83 (44) means that:

	
	- port reception facilities meet the needs of ships using ports without undue delay;

	
	- used by seafarers;

	
	- fully satisfy the needs of ships that regularly use them;

	
	- are not difficult to use, and contribute to the improvement of the state of the marine environment;

	
	- ensure the final disposal of shipboard waste in an environmentally sound way

	Quarantine waste
	Special ship wastes that require sorting and special handling due to their potential for the spread of diseases or pests of plants and animals

	Marine Terminal
	A set of port infrastructure facilities that are technologically interconnected and intended and (or) used to carry out operations with cargo, including for their transshipment, servicing ships, other vehicles and (or) serving passengers

	Garbage
	According to Annex V to the MARPOL Convention, these are all types of food, household and operational waste, all plastics, cargo residues, ash from incinerators, cooking oil, etc., which are formed during the normal operation of the vessel and are subject to periodic or permanent disposal, except for substances, the discharge of which is regulated by other Annexes to the MARPOL Convention

	Waste accumulation
	Waste accumulation in specially equipped places before it is sent to the waste disposal facility

	Waste management
	Activities for collection, accumulation, transportation, processing, disposal, disposal, disposal of waste

	Marine terminal operator
	A transport organization that operates the sea terminal, operations with cargo, including transshipment, servicing ships, other vehicles and (or) serving passengers

	Special Area
	A region of the world's oceans where, for recognized reasons relating to its oceanographic and ecological conditions

	Residue / Waste
	Refers to the totality of all MARPOL waste that is generated on board ships during normal operation and during cargo operations

	Transshipment of goods
	A complex type of services and (or) work on transshipment of goods from one type of transport to another, including the movement of goods within the seaport and their technological accumulation, or transshipment of goods without their technological accumulation from one type of transport to another type of transport

	Approaches to the seaport
	External roads and sections of sea routes located in a zone with established boundaries, which adjoins the seaport water area, but does not go beyond the territorial sea of ​​the Russian Federation, and within which vessels must navigate with particular caution in order to ensure the safety of navigation

	Port hydrotechnical facilities
	Engineering and technical structures: coastal protection, breakwaters, dams, breakwaters, piers, berths, as well as approach channels located on the territory and (or) water area of ​​the seaport, designed to ensure the safety of navigation and anchorage of ships

	Reception facility
	Fixed, floating or mobile facility designed to receive residues / waste from ships and which is suitable for this purpose

	Waste disposal
	Waste storage and disposal activities

	Discharge
	Means any discharge from a ship, whatever the cause, and includes any leak, disposal, spill, leak, pumping, release or emptying. In this document, the term “discharge” refers to those types of discharges that are foreseen and regulated in the MARPOL Convention

	Ship waste
	Useless, unnecessary or surplus substance that must be removed from the ship

	Services in the seaport
	Services, the provision of which to users is usually carried out in the seaport and on the approaches to it in accordance with international treaties of the Russian Federation and the legislation of the Russian Federation

	Waste storage
	Waste storage at specialized facilities - landfills for more than eleven months



[bookmark: _Toc216966731]3. Normative legal acts

[bookmark: _Toc216966732]3.1 International documents

	International Convention for the Prevention of Pollution of the Marine Environment from Ships, 1973, as amended by the 1978 Protocol in part:
- Annex I Regulations for the Prevention of Pollution by Oil.
- Annex II Regulations for the Control of Pollution by Noxious Liquid Substances in Bulk.
- Annex IV Regulations for the Prevention of Pollution by Wastewater.
- Annex V Regulations for the Prevention of Pollution by Garbage.
- Appendix VI Rules for the Prevention of Air Pollution.
- Regulation 12, Appendix I of IC MARPOL, regarding the requirements for facilities to provide oil terminals with facilities sufficient to receive and handle dirty and clean ballast, wash water from oil tankers, as well as reception facilities sufficient to receive other residues and oily mixtures ...
- Regulation 12, Appendix IV of IC MARPOL, regarding the requirements for providing seaports with reception facilities for the removal of wastewater from ships.
- Regulation 8, Appendix V of IC MARPOL, regarding the requirements for providing seaports with reception facilities for receiving garbage from ships.
- MEPC Guidance 83 (44) on ensuring the adequacy of port reception facilities for shipboard waste.
- Guidelines for the Use of Shore Devices and Waste Reception and Treatment Facilities (MEPC (35th session) 1994).
- IMO Guidelines for Port Reception Facility Service Providers and their Users (MEPC.1 / 834) 2014
- 2011 Guidelines for Reception Facilities under Annex VI of IC MARPOL (MEPC Resolution 199 (62)).
- Guidelines for Ship Sanitation (WHO 2013).

[bookmark: _Toc216966733]3.2 Normative legal acts of the Russian Federation

- Merchant Shipping Code of the Russian Federation of 30.04.1999 N81-FZ.
- Federal Law of 08.11.2007 N 261-FZ "On seaports in the Russian Federation and on amendments to certain legislative acts of the Russian Federation."
- Water Code of the Russian Federation "dated June 3, 2006 N 74-FZ.
- Federal Law of 10.01.2002 N 7-ФЗ "On Environmental Protection".
- Federal Law No. 89-FZ of 24.06.1998 "On Production and Consumption Wastes" in terms of "garbage reform", including separate collection and recycling of waste.
- Federal Law of 04.05.1999 N 96-FZ "On the protection of atmospheric air."
- Federal Law of 04.05.2011 N 99-FZ "On licensing certain types of activities."
- Decree of the Government of the Russian Federation of 12.11.2016 No. 1156 "On the management of solid municipal waste and amending the Decree of the Government of the Russian Federation of August 25, 2008 No. 641".
- Order of Rosprirodnadzor dated May 22, 2017 No. 242 "On approval of the Federal classification catalog of waste".
- Order of the Ministry of Transport of Russia dated October 26, 2017 No. 463 "On approval of the General rules for navigation and anchorage of ships in the seaports of the Russian Federation and on approaches to them."
- Order of the Ministry of Transport of Russia dated 21.08.2012 No. 324 "Mandatory regulations in the seaport of Yeysk".
- "Rules of Conducting Work on Cleaning the Contaminated Port Water Areas" (RD 31.04.01-90), approved by By letter of the MMF No. 29 dated 19.03.90.

[bookmark: _Toc216966734]4. Introduction

	This Plan is developed and intended for masters / shipowners / ship agents and operators of port reception facilities to describe the basic principles to be taken into account when transferring and receiving MARPOL residues / wastes.
	The plan takes into account the current legislation on production and consumption waste management, state regulation of port activities and the fulfillment of the international obligations of the Russian Federation in the field of merchant shipping, in order to ensure the adequacy of reception facilities for the removal of waste from ships in the port of Yeysk.
	The function of state supervision and control over the activities of operators of port reception facilities, the conditions for maintaining facilities for the placement and disposal of ship waste is carried out by specially authorized executive bodies on the basis of the current legislation of the Russian Federation. The captain of the seaport of Yeysk manages measures to prevent pollution of the seaport water area with industrial and consumer waste, sewage and (or) oily waters, oil and other hazardous and (or) substances harmful to human health and (or) the environment and eliminate the consequences of such pollution.
	The activities of operators of port reception facilities of enterprises providing environmental services to ships related to the placement and disposal of shipboard waste are carried out on a commercial basis within the framework of the current legislation of the Russian Federation.
	The plan reflects the formation of technological conditions for the removal and disposal of shipboard waste generated during the normal operation of ships, as well as other wastes, including those related to cargo, in the scope of compliance with MARPOL, port and national regulations.
	The procedures recommended by the Plan are aimed at ship-to-shore interaction and include reporting procedures, as well as the use of standard forms of documentation.
	The ship-generated waste management plan in the seaport of Yeysk is regularly updated in accordance with the information provided by the operators of the port reception facilities.
[bookmark: _Toc216966735]5. Purpose and objectives of the Plan
[bookmark: _Toc216966736]5.1 Main objectives of the Plan

	The main purposes of the Plan are:
fulfillment of the obligations stipulated by the conventions recognized by the Russian Federation in the field of preventing environmental pollution by wastes from ships in the seaport of Yeysk, aimed at maintaining the standard readiness and sufficiency of the port's technical means for the removal and disposal of ship waste;
adoption of measures aimed at the future development and modernization of port reception facilities;
prevention of dumping of ship wastes;
simplification of measures to fulfill the requests of ship agents for the removal and placement of all types of ship waste, including cargo residues, prevention of the forced idle time of ships while waiting or non-fulfillment of requests for waste removal;
control over the accumulation of ship waste when ships are staying in the seaport in order to prevent their excess accumulation by the time the ship is registered to leave the port.
[bookmark: _Toc216966737]5.2 Main objectives of the Plan
	The main objectives of the Plan are:
monitoring the technical means of operators of port reception facilities and the fulfillment of applications for types of work to remove waste from ships;
control over the accumulation of ship waste in the process of registration of ship arrivals / wastes and during their stay in the port;
justification of the need for the long-term development of reception facilities;
verification of applications in cases of refusal to fulfill the applications of ships for the performance of services for the removal of ship waste.
	The implementation of the goals and objectives of the plan is achieved subject to the conditions of interaction with state administration and control bodies in the field of environmental protection, control and supervisory bodies of sanitary, veterinary, phytosanitary control, economic relations and tariff policy, including special cases due to the circumstances of the introduction of a quarantine regime.

[bookmark: _Toc216966738]6. The main characteristics of the seaport of Yeysk

	The seaport of Yeysk is located in the Azov Sea on the southern coast of the Taganrog Bay.
	The boundaries of the seaport are established by the order of the Government of the Russian Federation dated April 22, 2009 N 549-r.
	The seaport is open for navigation all year round, operates around the clock, and has a permanent multilateral cargo checkpoint across the state border of the Russian Federation.
	In the seaport of Yeysk, 6 operators of sea terminals carry out operations with cargo, including transshipment, servicing ships and other vehicles:
- JSC "Yeisk Sea Port";
- JSC "Yeisk port elevator";
- LLC "Yeisk-port-Vista";
- LLC "Yeisk-Priazovye-Port";
- Yeisk Department of the Azov-Black Sea Basin Branch of FSUE "Rosmorport".
	Services for the removal of ship waste in the seaport of Yeysk are rendered by the operators of the port reception facilities LLC EcoLider and LLC Germes (Appendix 4).
[bookmark: _Toc216966739]7. Scheme of the port area and location of berths
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[bookmark: _Toc216966740]8. Characteristics of berths

Main technical characteristics of the seaport:
Seaport area (ha): 68.61
Seaport water area (km2): 63.39
Number of berths: 16
Length of the seaport mooring front (rm): 2 762
Through put of cargo terminals in total (thousand tons per year): 6 953.3
including:
liquid (thousand tons per year): 1 200
dry (thousand tons per year): 5,753.3
Maximum dimensions of vessels calling at the port (draft, length, width) (m): 4.5 / 150/22
Covered warehouse area (thousand m2): 42.45
Open warehouse area (thousand m2): 118.03
Storage tank capacities: grain (thousand tons): 77.4
Navigation period in the seaport: year-round
[bookmark: _Toc216966741]9. Characteristics of the composition of ship waste

	Inventory of ship waste generation, certification by types and classifiers of waste toxicity, limits on placement and responsibility for maintaining established payments for their generation and disposal are the responsibilities of operators of port reception facilities that provide environmental services to ships.
Ship wastes, according to Annex V of the MARPOL MC, are subject to separate accumulation and transfer to reception facilities according to the following types and categories:
MARPOL Annex I-related
Oily bilge water
Oily residues (sludge)
Oily tank washings
Dirty ballast water
Scale and sludge from tank cleaning

MARPOL Annex II–related Category of NLS  residue/water mixture for discharge to facility from tank washings:
Category X substance
Category Y substance
Category Z substance

MARPOL Annex IV–related
Sewage

MARPOL Annex V–related

A. Plastics
B. Food wastes
C. Domestic wastes
D. Cooking oil
E. Incinerator ashes
F. Operational wastes
G. Animal carcasses
G. Cargo residues dry
H. Fishing gear
I. E-waste
J. Cargo residues (non HME)
K. Cargo residues (HME)

MARPOL Annex VI–related
a. Ozone-depleting substances and equipment containing such substances
b. Exhaust gas-cleaning residues

Ballast Water Management (BWM) Convention–related
Ballast Water (BWM Convention)
Sediments (BWM Convention)

	Water after washing tanks ("slops") - water contaminated with oil products that was used to wash cargo tanks, that is, this type of waste is defined as associated with the cargo. Tankers that use crude oil to wash their tanks are handed over as cargo at the discharge port.
	Chemicals transported in bulk in the seaport of Yeysk are not transshipped.
	Discharge of wastewater treated by an installation approved by the classification society is allowed if its purification and disinfection performance meets the standards for the coli index no more than 2500, for BOD-5 - no more than 50 mg / l, for suspended solids - no more than 100 mg / l in excess of the content of suspended solids in flushing water is allowed in port waters in agreement with the sanitary authorities, if it is not of a salvo nature. In other cases, wastewater is subject to accumulation with subsequent delivery to reception facilities. According to epidemiological indications and according to the order of the sanitary authorities, the normatively treated ship's wastewater may also be prohibited from being discharged into port waters or being delivered to reception facilities.
	The conditions for the discharge of isolated ballast are regulated by the "International Convention for the Control and Management of Ships' Ballast Water and Sediments", set out in the "Mandatory Regulations in the Seaport of Yeysk". Vessels are allowed to discharge isolated ballast at the berth if the ballast was changed in the Sea of Azov, as there is an entry in the logbook.

[bookmark: _Toc216966742]10. Special ship wastes

	In the seaport of Yeysk, the requirements for the special treatment of certain types of ship wastes must be met (for example, the implementation of measures to prevent the spread of African swine fever, during quarantine). In cases of ships entering the port of Yeysk from epidemiologically unfavorable areas, operators of port reception facilities must ensure the safe removal, transportation and decontamination of all special ship waste from such ships by ashing in incinerators.

[bookmark: _Toc216966743]11. Calculation of the capacity of reception facilities

	A transport vessel, as an extraterritorial object, is not provided for the application of national procedures for the inventory of production and consumption wastes, their certification by hazard classes, rationing and obtaining limits for their maximum formation and placement, as well as making payments for emissions and discharges and waste disposal for everything. the time the vessel is in the territorial waters of the Russian Federation.
	According to the accounting data of the ship's waste removed by operators of port reception facilities, taking into account 5% of the stock, the capacity of port reception facilities in annual terms by waste types is:
	Household waste (m3) MARPOL Annex V–related 
	390

	Waste water (m3) MARPOL Annex IV–related  
	5300

	Bilge oily water and oil sludge (m3) MARPOL Annex I-related 
	2100



[bookmark: _Toc216966744]12. Procedure for the delivery of ship waste, documentation

	Removal of all types of ship waste is carried out within the framework of economic agreements between ship agents and operators of port reception facilities. At the same time, the duties of the ship agents include the provision of duly completed applications to the operators of the port reception facilities, and from the operators of the port reception facilities - the issuance of a certificate of the delivery of ship waste.
Ships en route to port shall send, through the ship's agent, prior notification of their intention to use port reception facilities by e-mail smbampe@mail.ru in accordance with the Guidelines for Adequacy of Port Reception Facilities for Ship Waste (resolution MEPC.83 (44)) 24 hours before arrival in port or immediately after departure from the previous port, if the duration of the voyage is less than 24 hours (Appendix No. 2).
	When submitting information about a ship's call to the seaport in the information system "PortControl", the ship's agent fills in clause 33 "The required amount of required waste delivery and their name" in accordance with the planned operations for the delivery of ship waste (name, quantity).
	To remove from the vessel the accumulated residues of oil products, bilge, utility and fecal waters, garbage, an application through the ship's agent is submitted to the operator of the port reception facilities, which provides waste collection services.
	During the transfer of MARPOL residues / wastes, appropriate procedures must be followed on board to prevent pollution of the environment.
	Shipboard waste is delivered at the berths of the seaport of Yeysk. Oily waters, as well as oil residues from ships are handed over at the port berths in a closed way. Standard dimensions of flanges and drain connections should ensure a reliable ship-to-reception connection.
	Upon completion of the removal of ship-generated waste, the operator of the port reception facilities shall issue the person responsible for the delivery of ship-generated waste on the ship with a certificate of the removal of ship-generated waste indicating the date, name and amount of the type of waste delivered (Appendix 3). Relevant records, certificates, receipts or certificates for the delivery of shipboard waste should be kept in the Garbage Record Book (for at least two years) and the Oil Record Book (Part I for all types of ships and Part II for oil tankers), and in the case of tankers for the transport of chemicals - in the Journal of Cargo Operations. The valves after the delivery of the ship's liquid waste must be sealed with the seals of the operator of the port reception facilities.
	When registering a ship's departure from the seaport, the ship's captain through the ship's agent submits to the seaport captain's service a certificate of the ship's waste delivery. In the event that the ship's waste was not removed from the ship, objective evidence must be provided that the volumes of the containers for the collection of ship's waste allow the passage to the next port of call or discharge in the permitted area in compliance with the requirements of MK MARPOL 73/78.
	For violations that would result in environmental pollution, the guilty party is subject to a fine and recovery of damage for causing harm to the natural environment in accordance with the Law of the Russian Federation "On Environmental Protection" No. 7-FZ of 10.01.02 and the current legislation of the Russian Federation. The imposition of penalties does not relieve the guilty party from paying the cost of the actual costs of eliminating environmental pollution.

[bookmark: _Toc216966745]13. Minimization of harmful effects on the environment in the management of residues / waste generated on the ship

	Household waste, pre-divided by type and category on the ship, is packed and transferred to the port reception facilities. In some cases, as prescribed by the sanitary authorities, household waste from ships, for epidemiological reasons, must be decontaminated on board, hermetically packed and then incinerated in an incinerator. The crew of the vessel makes appropriate records of the delivery of residues / waste in the Oil Record Book, Cargo Record Book and Garbage Record Book.

[bookmark: _Toc216966746]14. The main composition of technical means and the procedure for the movement of waste

	In the seaport of Yeysk, ship waste removal services are rendered by OOO EcoLider and OOO Germes (Appendix 4).
	Information about the port reception facilities of the seaport of Yeysk is formed on the basis of information provided by the operators of the port reception facilities and is available on the website of the Yeisk branch of the FSBI "AMP of the Sea of Azov": http://eisk.azovseaports.ru/kapitan_porta/ekologiya/f2750.html Database on port reception facilities was created within the framework of the Global Integrated Ship Information System (GISIS). Ship masters / shipowners / operators can use both the database of the GISIS website and the website of the Yeisk branch of the FSBI "AMP of the Sea of Azov" to obtain information about the reception facilities of the seaport of Yeysk. Operators of port reception facilities annually by July 15, and in the event of a change in the basic composition of technical means and waste flow patterns, within 10 days, provide information about their facilities, structures, contracts for final disposal, etc. to the captain of the seaport of Yeysk to update the ship's waste management plan to ensure its availability for ship masters, ship owners and ship agents.

[bookmark: _Toc216966747]14.1 Procedure for the movement of ship-generated waste when fulfilling the requirements of Annex I of MARPOL 73/78 (Rules for the Prevention of Oil Pollution)

[bookmark: _Toc216966748]14.1.1 Actions of the operator of port reception facilities LLC "Hermes"

	Specialized machines for the transportation of oily waters of the operator of port reception facilities LLC "Hermes" take from ships water containing oil products and deliver them for neutralization to the flotation unit № 03-0161-003312-Пof LLC "Hermes" in Yeysk, st.Michurin, 2a.
	Specialized machines of the operator of the port reception facilities LLC "Hermes" take oil sludge, waste oil and oil waste from ships and from the flotation unit, deliver and transfer them for disposal by LLC "Monolit", Timashevskst.Bavarskaya, 7 letters G8, G9 and LLC "Agency" Mercury Safety ", Art. Kholmskaya, Krasnodar Territory, Abinsky District.

[bookmark: _Toc216966749]14.1.2 Actions of the operator of port reception facilities LLC "EcoLider"

	Specialized machines for the transportation of oily waters of the operator of port reception facilities LLC "EcoLider" take water containing oil products from ships and deliver them to the production site of LLC "EcoLider" with accumulation tanks № 03-0223-004381-Пin Yeisk, st.Rabochaya, 2d, and then they are handed over for disposal by Monolit LLC, Timashevsk, Bavarskaya str., 7 letters G8, G9.
	Specialized machines of the operator of port reception facilities LLC "EcoLider" receive oil sludge, waste oil and oil waste from ships, deliver and transfer them for disposal by LLC "Monolit", Timashevsk, Bavarskayast., 7 letters G8, G9.

[bookmark: _Toc216966750]14.2 Procedure for the movement of ship-generated waste while meeting the requirements of Annex IV of MARPOL 73/78 Rules for the Prevention of Pollution by Waste Water
	Specialized machines for the transportation of wastewater of operators of port reception facilities LLC "EcoLider" and LLC "Germes" receive sewage and fecal waters from ships, take neutralized oily water from the flotation unit, deliver and transfer them for disposal to treatment facilities through a centralized drainage system to points of reception of the State Unitary Enterprise of the Krasnodar Territory "Kubanvodkompleks".

[bookmark: _Toc216966751]14.3 Procedure for the movement of ship-generated waste in compliance with the requirements of Annex V ofMARPOL 73/78 Garbage.
	Specialized vehicles for the transportation of solid municipal waste of operators of port reception facilities LLC "EcoLider" and LLC "Germes" take garbage from ships, deliver and transfer it for processing, neutralization and burial to the regional operator LLC "Chistayastanitsa", art. Leningradskaya. Number of the waste disposal facility is 23-00101-3-00371-2707174.
	The address of the location of the object is 353670, Krasnodar Territory, Yeisk district, Krasnoarmeyskoe rural settlement, 2nd km north of the village Simonovka.

[bookmark: _Toc216966752]15. Availability of operators of port reception facilities

	Port reception facility operators ensure that their equipment is in good condition and must be adequately prepared to receive ship's residues / waste. Reception procedures for sorted residues / waste should be in accordance with ISO 21070 standards for shipboard waste management and recycling.
	Port reception facility operators must have valid contracts with the regional MSW operator, wastewater treatment facility operator and petroleum waste disposal / disposal service provider, confirming the final disposal of shipboard waste.

[bookmark: _Toc216966753]16. Fee for reception and disposal of waste

	Port reception facilities should be provided at a reasonable, reasonable cost and not impede or restrict seafarers from using such services. Payment for the reception and disposal of waste is carried out on request through the ship's agent in accordance with the contract.

[bookmark: _Toc216966754]17. Government regulation

[bookmark: _Toc216966755]	17.1 Control by the Yeisk branch of the FSBI "AMP of the Azov Sea"
In accordance with Federal Law No. 261-FZ of 08.11.2007 "On seaports and amendments to certain legislative acts of the Russian Federation" quarantine, quarantine phytosanitary, veterinary, ecological and other types of state control (supervision) provided for by the legislation of the Russian Federation; manages measures to prevent pollution of the seaport water area with production and consumption waste, waste and (or) oily waters, oil and other substances hazardous and (or) harmful to human health and (or) the environment and eliminate the consequences of such pollution.
The duty of taking into account the sufficiency of port reception facilities by the port authorities is assigned to the leading specialist of the group for organizing work in the seaport of Yeysk and on the approaches to it of the Harbor Master's Service.
Verification of documents related to the execution of this plan by the vessels is carried out by the Captain's Service of the seaport of Yeysk, including when registering the arrival / departure of the vessel.
If the vessel fails to comply with the requirements of MK MARPOL 73/78 on the delivery of waste, in accordance with Art. 80 of the Merchant Shipping Code, the captain of the seaport has the right to refuse to issue a permit for the ship to leave the seaport in the event of a threat of damage to the marine environment or an order of the sanitary and quarantine service.
[bookmark: _Toc216966756]	17.2 Control by state control and supervisory authorities
Control actions in relation to shipboard waste within their competence are carried out by the Yeisk customs post.The epidemiological threat that can be posed from ships is determined and controlled by the Territorial Department of the Rospotrebnadzor Administration of the Krasnodar Territory in the Yeisk, Shcherbinovskiy and Starominskiy districts (Rospotrebnadzor).

[bookmark: _Toc216966757]18. Special and emission control areas
	The Black Sea and the Sea of Azov and their bays are considered special areas in this plan, where, for recognized reasons related to oceanographic and environmental conditions and the specifics of shipping, it is necessary to adopt special mandatory methods to prevent sea pollution by oil, other harmful substances and garbage.

[bookmark: _Toc216966758]19. Measures to prevent pollution of the water by liquid ship wastes
	In the water area of the seaport of Yeysk, it is prohibited to: discharge overboard any types of oily water, household waste water, water used to wash the deck, holds, cargo and bunker tanks, throw overboard food and other waste, any cargo and garbage residues.
According to the requirements of the International Convention for the Control and Management of Ships' Ballast Water and Sediments (BWM Convention), ships traveling to the seaport from the sea should replace the isolated ballast in the Black Sea in front of the Kerch Strait and in the Sea of Azov.
	Discharge of petroleum products, substances harmful to human health and wastewater within the port water area is prohibited. The master of the vessel is obliged to take all measures to prevent their spill. All cases of pollution of the port water area from his ship or upon detection of oil products on the surface of the water, the captain of the ship must immediately report this to port authorities and keep firefighting measures.
	Cleaning of the port water area mustcarry out at the expense of the perpetrators. The use of dispersants for cleaning the port water area without the approval and permission of state environmental and sanitary control is prohibited.
	When a ship approaches from seaward, the discharge valves of wastewater systems must be closed and sealed with a ship's seal.
	After the delivery of liquid waste at the berth to a specialized collector tanker, all shut-off valves of the ship must be sealed with the seals of the operator providing these services.
	In the case of washing the holds before loading, after unloading, the vessels must deliver the used water to a specialized vehicle.

[bookmark: _Toc216966759]20. Actions in case of dumping of oily waste
	In the event that oily ship waste is discharged into the water area of the seaport of Yeysk, cleaning work should be carried out in accordance with the Russian Federation Regulation "Rules for cleaning contaminated port water areas" RD 31.04.01-90, which establish a set of organizational, technical and technological requirements and recommendations for conducting work on cleaning of polluted port waters from floating impurities and oil spill response.
Information about the spill should be immediately transmitted to port authorities.
	In all cases of pollution of the port water area from his vessel or upon detection of oil products on the surface of the water, the captain of the vessel is obliged to immediately report an incident causing oil pollution to port authorities and take other actions in accordance with the Ship's Muster plan for oil pollution.

[bookmark: _Toc216966760]21. Reports on the lack of facilities for receiving ship waste
	In accordance with IMO Resolution MEPC 44/20 Annex 2 of the International Convention MARPOL 73/78 "Guidelines for Ensuring the Adequacy of Port Reception Facilities" by the owners or masters of ships, upon detection of an apparent inadequacy of port reception facilities, a report is drawn up in accordance with MEPC / Circ.349, which is transmitted The “flag state”, which in turn informs the “port state” and the IMO Secretariat.


[bookmark: _Toc216966761]Appendix 1 (FORMAT FOR REPORTING ALLEGED INADEQUACIES OF PORT RECEPTION FACILITIES)

FORMAT FOR REPORTING ALLEGED INADEQUACIES OF PORT RECEPTION FACILITIES *1
The master of a ship having encountered difficulties in discharging waste to reception facilities should forward the information below, together with any supporting documentation, to the Administration of the flag State and, if possible, to the competent Authorities in the port State. The flag State shall notify IMO and the port State of the occurrence. The port State should consider the report and respond appropriately informing IMO and the reporting flag State of the outcome of its investigation.


1	SHIP'S PARTICULARS
1.1	Name of ship:			_________________________
1.2	Owner or operator:		_________________________
1.3	Distinctive number or letters:	_________________________
1.4	IMO Number *2:			_________________________
1.5	Gross tonnage:			_________________________
1.6	Port of registry:			_________________________
1.7	Flag State *3:			_________________________
1.8	Type of ship:
	• Oil tanker		• Chemical tanker	• Bulk carrier
	• Other cargo ship	• Passenger ship	• Other (specify) ___________

2	PORT PARTICULARS
2.1	Country:				_________________________
2.2	Name of port or area:		_________________________
2.3	Location/terminal name:		_________________________
(e.g. berth/terminal/jetty)
2.4	Name of company operating
the reception facility (if applicable):	_________________________
2.5	Type of port operation:
	• Unloading port		• Loading port		• Shipyard
	• Other (specify) ___________________________
2.6	Date of arrival:		__/__/____ (dd/mm/yyyy)
2.7	Date of occurrence:	__/__/____ (dd/mm/yyyy)
2.8	Date of departure:	__/__/____ (dd/mm/yyyy)
_____________
*1	This format was approved by MEPC 53.
*2 	In accordance with the IMO ship identification number scheme, adopted by the Organization by Assembly resolution A.1117(30).
*3 	The name of the State whose flag the ship is entitled to fly.


INADEQUACY OF FACILITIES
Type and amount of wastes/residues for which the port reception facility was inadequate and nature of problems encountered
	Type of wastes/residues
	Amount for discharge (m3)
	Amount not accepted (m3)
	Problems encountered
Indicate the problems encountered by using one or more of the following code letters, as appropriate.
A No facility available
B Undue delay
C  Use of facility technically not possible
D Inconvenient location
E Ships had to shift berth involving delay/cost
F Unreasonable charges for use of facilities
G Other (please specify in paragraph 3.2)

	MARPOL Annex I-related
	
	
	

	Oily bilge water
	
	
	

	Oily residues (sludge)
	
	
	

	Oily tank washings
	
	
	

	Dirty ballast water
	
	
	

	Scale and sludge from tank cleaning
	
	
	

	Other
	
	
	

	MARPOL Annex II–related Category of NLS  residue/water mixture for discharge to facility from tank washings:
	
	
	

	Category X substance
	
	
	

	Category Y substance
	
	
	

	Category Z substance
	
	
	

	MARPOL Annex IV–related
	
	
	

	Sewage
	
	
	

	MARPOL Annex V–related
	
	
	

	A.  Plastics
	
	
	

	B. Food wastes
	
	
	

	C. Domestic wastes
	
	
	

	D. Cooking oil
	
	
	

	E. Incinerator ashes
	
	
	

	F. Operational wastes
	
	
	

	G. Animal carcasses
	
	
	

	H. Fishinggear
	
	
	

	I. E-waste
	
	
	

	J. Cargo residues (non HME)
	
	
	

	K. Cargoresidues (HME)
	
	
	

	MARPOL Annex VI–related
	
	
	

	a. Ozone-depleting substances and equipment containing such substances
	
	
	

	b. Exhaust gas-cleaning residues
	
	
	


___________
*4 Indicate, in paragraph 3.2, the proper shipping name of the NLS involved and whether the substance is designated as "solidifying" or "high viscosity" as per MARPOL Annex II, regulation 1, paragraphs 15.1 and 17.1 respectively.
*5 Indicate the proper shipping name of the dry cargo.

3.2 Additional information with regard to the problems identified in the above table
___________________________________________________________________
___________________________________________________________________
___________________________________________________________________
___________________________________________________________________
3.3 Did you discuss these problems or report them to the port reception facility?
 Yes 		 No
If Yes, with whom (please specify) ___________________________________________________________________ 
If Yes, what was the response of the port reception facility to your concerns? ___________________________________________________________________ 

	3.4 
	Did you give prior notification (in accordance with relevant port requirements) about the ship's requirements for reception facilities?


 Yes 		т No 		 Not applicable
If Yes, did you receive confirmation on the availability of reception facilities on arrival?
 Yes 		 No 	
4 
ADDITIONAL REMARKS/COMMENTS
___________________________________________________________________
___________________________________________________________________
Master's signature 		Date: __/__/____ (dd/mm/yyyy)


[bookmark: _Toc216966762]Appendix 2 STANDARD FORMAT OF THE ADVANCE NOTIFICATION FORM FOR WASTE DELIVERY TO PORT RECEPTION FACILITIES
p.1
[bookmark: _Toc80784503][bookmark: _Toc216966763]STANDARD FORMAT OF THE ADVANCE NOTIFICATION FORM FOR WASTE DELIVERY TO PORT RECEPTION FACILITIES

Notification of the Delivery of Wastes/Residues to: …………….…..…………………….. (enter name of port or terminal)
The master of a ship should forward the information below to the designated authority at least 24 hours in advance of arrival or upon departure of the previous port if the voyage is less than 24 hours.
This form should be retained on board the ship along with the appropriate Oil Record Book, Cargo Record Book or Garbage Record Book.
DELIVERY FROM SHIPS (ANF)
1. SHIP PARTICULARS
	1.1. Name of ship:
	1.5. Owneroroperator:

	1.2. IMO number:
	1.6. Distinctive number or letters:

	1.3. Gross tonnage:
	1.7. Flag State:

	[bookmark: %25D0%25A4%25D0%25BB%25D0%25B0%25D0%25B6][bookmark: __Fieldmark__0_358720262][bookmark: __Fieldmark__1_358720262][bookmark: __Fieldmark__2_358720262]1.4. Type of ship::   |_| Oil tanker      |_| Chemical tanker     
[bookmark: __Fieldmark__3_358720262][bookmark: __Fieldmark__4_358720262][bookmark: __Fieldmark__5_358720262]|_|   Bulk carrier     |_| Container      |_| Other cargo ship    
[bookmark: __Fieldmark__6_358720262][bookmark: __Fieldmark__7_358720262]|_| Passenger ship  |_| Ro-ro      |_| Other (specify)



2. PORT AND VOYAGE PARTICULARS
	2.1. Location/Terminal name and POC:
	2.6.: Last Port where wastes/residues were delivered:

	2.2. Arrival Date and Time:
	2.7. Date of Last Delivery:

	2.3. Departure Date and Time:
	2.8. Next Port of Delivery (if known):

	2.4. Last Port and Country:
	2.9. Person submitting this form is (if other than the master):

	2.5. Next Port and Country (if known):
	



3. ВИД И КОЛИЧЕСТВО ОТХОДОВ СДАВАЕМЫХ НА ПРИЕМНЫЕ СООРУЖЕНИЯ
	MARPOL Annex I-related
	Amount (m3)
	
	MARPOL Annex V–related
	Amount (m3)

	Oily bilge water
	 
	
	A. Plastics
	 

	Oily residues (sludge)
	 
	
	B. Food wastes
	 

	Oily tank washings
	 
	
	C. Domestic wastes
	 

	Dirty ballast water
	 
	
	D. Cooking oil
	 

	Scale and sludge from tank cleaning
	 
	
	E. Incinerator ashes
	 

	Other
	 
	
	F. Operational wastes
	 

	
	
	G. Animal carcasses
	 

	MARPOL Annex II–related Category of NLS  residue/water mixture for discharge to facility from tank washings:
	Amount (m3) Shipping name
	
	H. Fishing gear
	 

	Category X substance
	 
	
	I. E-waste
	 

	Category Y substance
	 
	
	J. Cargo residues (non HME)
	 

	Category Z substance
	 
	
	K. Cargoresidues (HME)
	 

	
	
	MARPOL Annex VI–related
	Amount (m3)

	MARPOL Annex IV–related
	Amount (m3)
	
	a. Ozone-depleting substances and equipment containing such substances
	 

	Sewage
	 
	
	b. Exhaust gas-cleaning residues
	 


________________________________________________ 
1Indicate the proper shipping name	
2Indicate the proper shipping name of the dry cargo

MEPC.1/Circ.644/Rev.1
Приложение 2 , страница 2  p.2
	Name of ship:
	IMO number:


Please state below the approximate amount of wastes/residues remaining on board and the percentage of maximum storage capacity.If delivering all wastes/residues on board at this port please strike through this table and tick the box below. If delivering some or no waste/residue, please complete all columns.
[bookmark: __Fieldmark__8_358720262]I confirm that I am delivering all the wastes/residues held on board this vessel (as shown on page 1) at this port |_|
	Type
	Maximum dedicated  storage capacity (m3)
	Amount of wastes /residues retained on board (m3)
	Port at which remaining wastes/residues will be delivered (if known)
	Estimate amount of wastes/residues to be generated between notification and next port of call (m3)

	MARPOL Annex I-related

	Oily bilge water
	
	
	
	

	Oily residues (sludge)
	
	
	
	

	Oily tank washings
	
	
	
	

	Dirty ballast water
	
	
	
	

	/Scale and sludge from tank cleaning
	
	
	
	

	Other
	
	
	
	

	MARPOL Annex II–related Category of NLS  residue/water mixture for discharge to facility from tank washings:3

	Category X substance
	
	
	
	

	Category Y substance
	
	
	
	

	Category Z substance
	
	
	
	

	MARPOL Annex IV–related

	Sewage
	
	
	
	

	MARPOL Annex V–related

	A. Plastics
	
	
	
	

	B. Food wastes
	
	
	
	

	C. Domestic wastes
	
	
	
	

	D. Cooking oil
	
	
	
	

	E. Incinerator ashes
	
	
	
	

	F. Operational wastes
	
	
	
	

	G. Animal carcasses
	
	
	
	

	H. Fishing gear
	
	
	
	

	I. E-waste
	
	
	
	

	J. Cargo residues (non HME) 4
	
	
	
	

	K. Cargo residues (HME) 4
	
	
	
	

	MARPOL Annex VI–related

	a. Ozone-depleting substances and equipment containing such substances
	
	
	
	

	b. Exhaust gas-cleaning residues
	
	
	
	

	Date:
	
	
	Name:
	

	Time:
	
	
	Sign
	


_________________________________           
3Indicate the proper shipping name	
4Indicate the proper shipping name of the dry cargo
[bookmark: _Toc80784504][bookmark: _Toc216966764]
Appendix 3 Confirmation

Port Yeysk
CERTIFICATE №

This is to confirm that from m/v 		____________________________

Flag	__________________________________ 

Provider		_____________________________

has delivered on the car-collector					of total volume as indicate below
	Type
	Объем выгрузки (м3)Amount (m3)
	
	Type
	Amount (m3)

	 MARPOL Annex I-related 
	
	 MARPOL Annex V–related 

	Oilybilgewater
	 
	
	A. Plastics
	 

	Oily residues (sludge)	
	 
	
	B. Food wastes
	 

	Oilytankwashings
	 
	
	C. Domestic wastes
	 

	Dirtyballastwater
	 
	
	D. Cooking oil
	 

	Scale and sludge from tank cleaning
	 
	
	E. Incinerator ashes
	 

	Other
	 
	
	F. Operationalwastes
	 

	MARPOL Annex II–related Category of NLS  residue/water mixture for discharge to facility from tank washings: 
	
	G. Animal carcasses
	 

	
	
	H. Fishing gear
	 

	Category X substance
	 
	
	I. E-waste
	 

	Category Y substance
	 
	
	J. Cargo residues (non HME)
	 

	Category Z substance
	 
	
	K. Cargoresidues (HME)
	 

	
	 
	
	MARPOL Annex VI–related 

	MARPOL Annex IV–related 
	
	a. Ozone-depleting substances and equipment containing such substances
	 

	Sewage
	 
	
	b. Exhaust gas-cleaning residues
	 



Commencement of service:              __________   __________     ___________________
	h	 min 		date

Completion of service:                  __________   __________     ___________________
	h	 min 		date

Total service time:                     __________   __________     ___________________
	h	 min 		date



	[bookmark: _Toc80784505][bookmark: _Toc216966765]Appendix 4Yeisk port reception facilities

Yeisk port reception facilities 

	1. MARPOL Annex I – related  
	

	
 Provider 
	Name
	 «EcoLider» Ltd
	“Germes” Ltd

	
	Address
	Yeisk
	Yeisk

	
	Telephone
	8-918-155-66-77
	(988) 966-02-02

	
	Telex
	−
	− 

	
	Fax
	(86132) 2-68-03
	− 

	
	Email
	planida.eysk@mail.ru
	goryain_gav@mail.ru 

	
	Website
	−
	− 

	 
Type of port reception facilities
	Choose one or more of:
	

	
	F (fixed) 
	F 
	F 

	
	T (tanker or barge) 
	−
	− 

	
	Tr (
 truck or portable tank) 
	Tr
	Tr

	
	
Other (specify)
	−
	− 

	
Restrictions on receipt or collection
	Minimum quantity (м3) 
	unlimited
	unlimited

	
	Maximum quantity (м3)
	unlimited
	80

	
	
Discharge rate (m3 /hour)
	20
	10

	
	
Other (specify)
	−
	− 

	
Reception facilities available
	24 hours a day, 7 days per week
	+
	+ 

	
	24 hours a day, 5 days per week
	−
	− 

	
	Business hours only, 7 days per week
	−
	− 

	
	Business hours only, 5 days per week
	−
	− 

	
	
Other (specify)
	−
	− 

	Prior notice for  receipt of oily wastes is required
	
(hours)
	2
	2

	
 Payment
	Choose one or more of:
	

	
	At no cost
	−
	− 

	
	
At a cost incorporated into standing port use charge
	−
	− 

	
	
At a cost charged in addition to other services
	+
	+ 

	
	
Other (specify)
	
	

	 IMO category:
	Oily bilge water
	+ 
	+ 

	
	Oily residues (sludge)
	+ 
	+ 

	
	Oily tank washings
	+ 
	+ 

	
	Dirty ballast water
	+ 
	+ 

	
	Scale and sludge from tank cleaning
	+ 
	+ 

	
	Other (specify)
	Including waste used oil
	Including waste used oil

	Comments:
	Needtoadd
	
	

	Lastupdate
	(data)
	07.07.2025
	17.12.2025





	2.  MARPOL Annex II–related Category of NLS  residue/water mixture for discharge to facility from tank washings

	 Provider
	Name
	− 

	
Lastupdate
	(data)
	07.07.2025




	3. Мусор. V / MARPOL Annex V – related
	

	
 Provider 
	Name
	«EcoLider» Ltd
	“Germes” Ltd

	
	Address
	Yeisk
	Yeisk

	
	Telephone
	8-918-155-66-77
	(988) 966-02-02

	
	Telex
	−
	− 

	
	Fax
	(86132) 2-68-03
	− 

	
	Email
	planida.eysk@mail.ru
	goryain_gav@mail.ru 

	
	Website
	−
	− 

	 
Type of port reception facilities
	Choose one or more of:
	

	
	F (/ fixed) 
	−
	− 

	
	T (tanker or barge) 
	−
	− 

	
	Tr ( truck or portable tank) 
	Tr
	Tr

	
	Other (specify)
	−
	− 

	
Restrictions on receipt or collection
	Minimum quantity (м3) 
	unlimited
	unlimited

	
	Maximum quantity (м3)
	unlimited
	unlimited

	
	Discharge rate (m3 /hour)
	10
	5

	
	Other (specify)
	−
	− 

	
Reception facilities available
	24 hours a day, 7 days per week
	+
	+ 

	
	24 hours a day, 5 days per week
	−
	− 

	
	Business hours only, 7 days per week
	−
	− 

	
	Business hours only, 5 days per week
	−
	− 

	
	Other (specify)
	−
	− 

	Prior notice for  receipt of oily wastes is required
	(hours)
	2
	2

	
 Payment
	Choose one of:
	

	
	At no cost
	−
	− 

	
	At a cost incorporated into standing port use charge
	−
	− 

	
	At a cost charged in addition to other services
	+
	+ 

	
	Other (specify)
	−
	− 

	
 IMO category:
	A. / Plastics
	+ 
	+ 

	
	B. Food wastes
	− 
	+ 

	
	C. Domestic wastes
	+ 
	+ 

	
	D. Cooking oil
	− 
	+ 

	
	E. Incinerator ashes
	+ 
	+ 

	
	F. Operational wastes
	+ 
	+ 

	
	G. Animal carcasses
	− 
	− 

	
	H. Fishing gear
	+ 
	+ 

	
	I. E−waste
	+ 
	+ 

	
	J. Cargo residues (non HME)
	+ 
	+ 

	
	K. Cargoresidues (HME)
	+ 
	+ 

	Comments:
	Need to add:
	− 
	− 

	Lastupdate
	(data)
	07.07.2025
	17.12.2025





	4. Сточныеводы. IV / MARPOL Annex IV – related 

	Provider
	Name
	«EcoLider» Ltd
	“Germes” Ltd

	
	Address
	Yeisk
	Yeisk

	
	Telephone
	8-918-155-66-77
	(988) 966-02-02

	
	Telex
	−
	− 

	
	Fax
	(86132) 2-68-03
	− 

	
	Email
	planida.eysk@mail.ru
	goryain_gav@mail.ru 

	
	Website
	−
	− 

	 
Type of port reception facilities
	Choose one or more of:
	

	
	F (/ fixed) 
	−
	− 

	
	T (tanker or barge) 
	−
	− 

	
	Tr ( truck or portable tank) 
	Tr
	Tr

	
	Other (specify)
	−
	− 

	
Restrictions on receipt or collection
	Minimum quantity (м3) 
	unlimited
	unlimited

	
	Maximum quantity (м3)
	unlimited
	unlimited

	
	Discharge rate (m3 /hour)
	20
	10

	
	Other (specify)
	−
	− 

	
Reception facilities available
	24 hours a day, 7 days per week
	+
	+ 

	
	24 hours a day, 5 days per week
	−
	− 

	
	Business hours only, 7 days per week
	−
	− 

	
	Business hours only, 5 days per week
	−
	− 

	
	Other (specify)
	−
	− 

	Prior notice for  receipt of oily wastes is required
	(hours)
	2
	2

	
 Payment
	Choose one of:
	

	
	At no cost
	−
	− 

	
	At a cost incorporated into standing port use charge
	−
	− 

	
	At a cost charged in addition to other services
	+
	+ 

	
	Other (specify)
	−
	

	Comments:
	Need to add:
	−
	−

	Lastupdate
	(дата) 
	07.07.2025
	17.12.2025





	5. MARPOL Annex VI – related 

	Provider
	Name
	− 

	Last update
	(data)
	07.07.2025



	6. BWM Convention-related 
	
	

	
 Provider 
	Name
	«EcoLider» Ltd
	«EcoLider» Ltd

	
	Address
	Yeisk
	Yeisk

	
	Telephone
	8-918-155-66-77
	8-918-155-66-77

	
	Telex
	−
	−

	
	Fax
	(86132) 2-68-03
	(86132) 2-68-03

	
	Email
	planida.eysk@mail.ru
	planida.eysk@mail.ru

	
	Website
	−
	−

	 
Type of port reception facilities
	Choose one or more of:
	
	

	
	F (fixed) 
	− 
	− 

	
	T (tanker or barge) 
	− 
	− 

	
	Tr (truck or portable tank) 
	Tr
	Tr

	
	Other (specify)
	− 
	− 

	
Restrictions on receipt or collection
	Minimum quantity (м3) 
	6
	−

	
	Maximum quantity (м3)
	30
	30

	
	Discharge rate (m3 /hour)
	6
	−

	
	Other (specify)
	
	

	
Reception facilities available
	24 hours a day, 7 days per week
	+
	+

	
	24 hours a day, 5 days per week
	
	

	
	Business hours only, 7 days per week
	
	

	
	Business hours only, 5 days per week
	
	

	
	Other (specify)
	
	

	Prior notice for  receipt of oily wastes is required
	(hours)
	2
	2

	
 Payment
	Choose one of:
	
	

	
	At no cost
	− 
	− 

	
	At a cost incorporated into standing port use charge
	− 
	− 

	
	At a cost charged in addition to other services
	+ 
	+ 

	
	Other (specify)
	
	

	Comments:
	Need to add:
	−
	−

	
	Ballast water (BWM Convention)
	− 
	− 

	
	Sediments (BWM Convention)
	+ 
	+ 

	Last update
	 (data)
	07.07.2025
	17.12.2025











[bookmark: _Toc216966766]Appendix 5 Sources of additional information

• International IMO Global Integrated Marine Information System (GISIS) website: http://gisis.imo.org/Public/
• Consolidated version of the Convention - includes all articles, protocols, annexes and unified interpretations: http://www.imo.org/Publications/mainframe.asp?topicJd=424 (product # ID520E)
• IMO 1999 Integrated Guide to Port Reception Facilities: http://www.imo.org/Publications/mainframe.asp?topicJd=424 (product # IA597E)
• MARPOL Annex V Implementation Guide 2012: http://www.imo.org/Publications/mainframe.asp?topicJd=424 (product # IB656E)
• Guidelines for the adequacy of port reception facilities for ship waste (resolution MEPC.83 (44)): http://www.imo.org/Publications/mainframe.asp?topicJd=424 (product # I598E).
• Article 78 of the Code of Merchant Navigation of the Russian Federation of April 30, 1999 No. 81-FZ
• Article 12 of the Federal Law of November 08, 2007On seaports of the Russian Federation and amendments to certain legislative acts of the Russian Federation"
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